
****



**Ceramic Finish Raised Floor**






**Abeite** Ceramic Finish Raised Floor is based on cold-rolled steel, high-density

calcium sulfate panel or chipboard. The bottom finished with galvanized steel sheet or

aluminum foil, etc covering. From the selection of materials, procurement, production,

packaging, are in accordance with the Chinese and PSA MOB PS/SPU、DIN EN 12825

specifications.





|  |  |
| --- | --- |
| Type: | FS662-1500 |
| Finished Floor Height: | 70-2000mm |
| Panel Size: | 600\*600mm、800\*800mm and special size |
| Ceramic Thickness: | 10/12mm |
| Ceramic Type: | Normal ceramic and Anti-static ceramic |

**Characteristics:**

1、Stable electrostatic performance, Class A fire, sound insulation, dust and dirt

resistance, chemical corrosion resistance；

2、Strong surface wear resistance, the hardness of 7 degrees Mohs, easy to clean；

3、No deformation, no dust, strong carrying capacity, combined with ceramic

characteristics, anti-aging, the service life of more than 60 years；

4、Variety of colors, including pure white, wood grain, etc., beautifully paved,

decorative；

5、OEM is available;

****

**Applications:**

Data Centers、Commercial Buildings、Educational Facilities、Clean Rooms、

Control Rooms、Libraries and places where require anti-static environment

or have many wires.




**Specification:**



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Type** | **Size** | **Concertrated Load Defleation≤2.5mm** | | | **Uniform Load** | **Ultimate Load** | **System Resistance** |
| **mm** | **LBS** | **KN** | **KG** | **KN/㎡** | **KN** | **Ω** |
| FS662 | 600\*600 | 662 | 2.95 | 300 | 12.50 | 8.85 | 1.0x106-1.0x109 |
| FS800 | 800 | 3.56 | 363 | 16.10 | 10.68 |
| FS1000 | 1000 | 4.45 | 454 | 23.00 | 13.35 |
| FS1250 | 1250 | 5.56 | 567 | 33.00 | 16.68 |
| FS1500 | 1500 | 6.67 | 680 | 34.50 | 20.02 |
| FS2000 | 2000 | 8.90 | 906 | 46.00 | 26.70 |

**Ceramic Color**

**.**

****



****

****

**Light gray Gray Heavy gray**

****



Changzhou Abeite Computer Room Equipment Co.,Ltd

Add: No. 108, Chaoyang Village, Hengshanqiao Town, Wujin District,

Changzhou City, Jiangsu Province，China

Tel: +86(519)86056270

Fax: +86(519)86056270

E-mail: info@abeiteraisedfloor.com

Web: www. abeiteraisedfloor.com