



**Glass Viewing Raised Floor**



**Abeite** Glass Viewing Raised Floor types fall into two categories: Tempered

Clear Glass and Tempered Laminated Glass. Glass panel can in combination with


steel raised floor, calcium sulfate raised floor, wood core raised floor and aluminum

raised floor.

The glass floor is not the simple tempered glass floor, but the world's leading

aviation special craft glass and aluminum alloy grinding tools. The rigidity and

toughness of the floor itself are the ultimate, and it is the safest transparent glass floor.

Beautiful, practical, generous, suitable for all kinds of computer room environment monitoring Indoor decoration Outdoor square landscape and other occasions. The anti-static transparent glass floor of the equipment room is used in all kinds of standard computer rooms, and the equipment, instruments, lines, and water leakage conditions

are checked 24 hours; The modern precision machine room needs to check the

running condition of the equipment at any time, and the conventional floor needs to

take off the original floor. It is very troublesome to use the high transparent anti-static glass floor. The glass floor has three requirements of high strength, beautiful and

practical, anti-static, and can be applied.

|  |  |
| --- | --- |
| Finished Floor Height: | 70-2000mm |
| Panel Size: | 600\*600mm、800\*800mm and special size |
| Tempered Clear Glass: | 12、15、19mm |
| Tempered Laminated Glass: | 10+10mm、10+12mm、12+12mm |



**Tempered glass** is a type of safety glass manufactured with the aid of heat or

chemicals used to strengthen the glass. This process is sometimes referred to as


“tempering.” Tempered glass can be up to four times stronger than typical annealed

glass of the same size and thickness.

Other benefits of tempered glass:

* More tensile strength (it can bend easier without breaking)
* Wind resistance
* If it breaks, tempered glass shatters into rounded cubes rather than pointy shards





**Laminated glass** is a type of safety glass that is made of two or more panes of

annealed glass joined together by a layer of plastic, or polyvinyl butyral (PVB).

You can think of this joining as creating a glass sandwich (glass, plastic, glass).

Some types of laminated glass are made with multiple layers (think of these as a

laminated glass layer cake).

Laminated glass features:

* The plastic portion of laminated glass may be clear or tinted.
* Laminated glass aids in the screening of UV radiation.
* Laminated glass is beneficial for soundproofing.

One of the biggest benefits of laminated glass is that if it does break, the broken

glass will stick to the plastic rather than falling to the floor.




**Applications:**

Data Centers、Educational Facilities、Clean Rooms、Control Rooms、Libraries

and places where request continuous monitor of underfloor equipment or environment.

****





Changzhou Abeite Computer Room Equipment Co.,Ltd

Add: No. 108, Chaoyang Village, Hengshanqiao Town, Wujin District,

Changzhou City, Jiangsu Province，China

Tel: +86(519)86056270

Fax: +86(519)86056270

E-mail: gail@abeiteraisedfloor.com

Web: www. abeiteraisedfloor.com