



**Airflow Perforated Raised Floor**



**Abeite** Airflow Perforated Raised Floor could in combination with steel raised

floor, calcium sulfate raised floor, wood core raised floor and aluminum raised floor.

Airflow perforated panel could cater to all your data center cooling needs, It use

the underfloor plenum for air supply or return and it takes advantage of natural thermal

lift with warm and stale air extracted by ceiling returns. This results in more pleasant

working conditions for human comfort. It is available in standard or heavy-duty load

ratings and surface coverings finish are tailored to match the finish of the solid panel.


|  |  |
| --- | --- |
| Ventilation Rate: | 15%-65% |
| Materials: | Steel、Aluminum |
| Panel Size: | 600\*600mm and other special size |
| Edge Trim Type: | Formal trim、Trimless |
| Finish Covering: | Bare with powder coated、1.0-2.0mm Anti-static Laminate HPL、2.0-3.0mm PVC、10mm Cermic and etc. |
| Damper: | Available |
| Installation: | With Stringer System |

****

Formal trim Trimless



****

****



**Damper Ceramic finish airflow panel**


****


**Special size airflow panel Adjustable height**



**Steel airflow panel**

****



**Ventilation Rate 15%**

**φ8mm \* 2048 pcs airflow hole**

**Ventilation Rate 20%**

**φ10mm \* 918 pcs airflow hole**



****

**Ventilation Rate 50%**

**200pcs airflow hole**

****



**Ventilation Rate 65%**

****





**Ventilation Rate 70%**

**Aluminum airflow panel**

****

**Ventilation Rate 55%**



****

**Ventilation Rate 15%**

****

**Ventilation Rate 35% Ventilation Rate 60%**

**Applications:**

All kinds of the computer room, communication room, monitoring and command

center, electronic factory clean room, switch room and other pipelines where air

circulation requirements are relatively concentrated and dustproof and anti-static.



Changzhou Abeite Computer Room Equipment Co.,Ltd

Add: No. 108, Chaoyang Village, Hengshanqiao Town, Wujin District,

Changzhou City, Jiangsu Province，China

Tel: +86(519)86056270

Fax: +86(519)86056270

E-mail: info@abeiteraisedfloor.com

Web: www. abeiteraisedfloor.com